Advanced Scanning / Optimizing Scanning

# Adjusting Color

> Adjusting the Gray Balance Intensity setting
> Adjusting the Saturation setting
> Making tone curve settings

Color adjustments should be made after adjusting settings related to brightness and contrast. Color settings should be made in the order shown above.

## Adjusting the Gray Balance Intensity setting

Gray Balance Intensity setting allows you to remove a cast (tint) from a specific color.

| Click the Color Adjustment button in the Manual mode window to open the Color Adjustment dialog box.

|  | Note:

The Color Adjustment button appears dimmed and these settings cannot be selected when Pixel Depth is set to 16-bit Gray, 8-bit Gray, or Black & White.

| In the Color Adjustment dialog box, click the eyedropper button under Gray Balance Intensity.

> The mouse pointer changes to an eyedropper, with movement restricted to within the Preview window.

|  | Note:

If you want to stop adjusting the setting using the eyedropper, press the ESC key on your keyboard.

| Move the eyedropper to a location where you want to adjust gray balance intensity, and then click.

> The color you selected appears in the two boxes below the Gray Balance Intensity slider.

| To change the gray balance intensity level of the color you selected, move the slider left or right, or enter a value in the text box.

set to 100

> You can enter a value between 0 and 100. Changing the value causes the color in the right hand box to change accordingly. Your changes are also reflected in the image in the Preview window.

| Note:

Click Cancel to restore the original image.

[Top]

## Adjusting the Saturation setting

Saturation is the density of a color. Higher saturation makes the color appear richer, while lower saturation makes it appear paler.

original image | set to 50

Follow these steps to adjust the Saturation setting.

| Click the Color Adjustment button in the Manual mode window.

| Move the Saturation slider left or right, or input a value between -100 (lowest color density) and 100 (highest color density).

[Top]

## Making tone curve settings

The tone curve provides you with a versatile means for adjusting the intensity of the colors of the image being scanned. You can adjust the shadow, mid-tone, and highlight values, which helps to ensure well-balanced coloring of the image.

| Note:

- Use of the tone curve is recommended for fine adjustments after you have previewed the image and adjusted the highlights and the shadows using Auto Exposure and the Image Controls dialog box. Use of the tone curve to make initial settings is not recommended.

- The Tone Correction button appears dimmed and is not available when Pixel Depth is set to Black & White and Halftone is set to None, or B/W Option is set to Text Enhancement Technology in the Image Type dialog box.

The tone curve is located in the Tone Correction dialog box, which appears when you click the Tone Correction button in the Manual mode window. The following section describes how to use each of the controls in the Tone Correction dialog box.

### Tone Curve Name list

Use this list box to select a preset tone curve. There are six preset tone curves available as shown below, and you can add your own curves to the list using the procedure in the next section, Saving your own tone curve.

Curve Name | Highlight | 1/4 Tone | Midtone | 3/4 Tone | Shadow | Description
Linear | 245 | 192 | 128 | 64 | 8 | Default curve
Lighten | 245 | 193 | 133 | 74 | 4 | Lightens dark image
Darken | 245 | 152 | 82 | 38 | 11 | Darkens bright image
Flat Contrast | 245 | 182 | 129 | 72 | 2 | Reduces contrast
High Contrast | 245 | 204 | 129 | 51 | 2 | Increases contrast
Open Shadow | 245 | 193 | 129 | 80 | 5 | Lightens dark shadows

When you select a curve from the Tone Curve Name list, the settings in the Tone Correction dialog box change accordingly.

| Note for Perfection 1260 and 1260 Photo users:

Open Shadow does not appear in the Tone Curve Name list.

### Channels

Click an option button under channels to select the color whose tone curve you want to adjust. When the master channel at the top is selected, your adjustments affect all three colors. Selecting one of the other channels allows you to adjust red, green, or blue only.

| Note:

If Pixel Depth is set to Black & White, 16-bit Gray, or 8-bit Gray in the Image Type dialog box, you can only select the combined RGB channel option.

### Tone curve editor

Moving the mouse pointer into the tone curve editor causes it to change to a finger. Use this pointer to drag any of the five points in the curve and change its shape. The x-axis of the curve is the brightness of the original (input values) while the y-axis is the brightness of the scanned image (output values).

To change the tone curve back to its default, select Linear from the Tone Curve Name list.

### Output values

These are the current values for output data in accordance with the current locations of the points inside the tone curve editor. These values change when you drag points in the tone curve editor, or you can enter values here to change the shape of the tone curve. Each value can be adjusted within the range of 0 to 255.

| Note:

- Each output value name has a check box to the left of it. Highlight and Shadow are always selected, but you can select or clear 1/4 Tone, Midtone, and 3/4 Tone by clicking their check boxes.

- When a value's check box is clear, its point on the tone curve editor automatically shifts to smooth out the tone curve when one of the other points is moved.

- When a value's check box is selected, it means that its point is fixed and it will not shift when other points are moved.

### Save/Delete/OK/Cancel/Help buttons

After you correct tone, type a name for your custom settings in the Tone Curve Name box and click Save.

To delete a setting, select the name of the setting you want to delete in the tone correction list and click Delete.

To apply the current Tone Correction dialog box settings and close the dialog box, click OK.

To cancel the operation and close the dialog box, click Cancel.

To access the online help, click Help.

### Customizing your own tone curve

#### Saving your own tone curve

Use the following procedure to assign a name to a tone curve you have customized and want to save for later use:

| Modify the tone curve settings as desired. This causes the name shown in the Tone Curve Name box to change to User Defined.

| After customizing the tone curve, enter a name for the new curve (up to 32 characters) in the list box.

| Click Save to save your new tone curve settings under the name you specified.

#### Deleting a customized tone curve

Use the following procedure to delete a custom tone curve. You cannot, however, delete the preset tone patterns.

| Use the Tone Curve Name list to select the custom tone curve you want to delete.

| Click Delete.

| When a dialog box appears, click Yes to delete the curve.

[Top]

Previous | Next