2017-07-16T15-00-03: LogOut_File: : logfile started
2017-07-16T15-00-03: Net Status: low-level initialize success.
2017-07-16T15-00-03: Note: this version (1/29/2017) has new data fields added
2017-07-16T15-00-03: time = time since start of game in ms.
2017-07-16T15-00-03: address = address of IP address
2017-07-16T15-00-03: incoming = total size of messages set to me in bytes. Spikes can indicate lag.
2017-07-16T15-00-03: outgoing = total size of messages set from me in bytes. Spikes can indicate lag.
2017-07-16T15-00-03: app_ctos = client to server bytes delta excluding overheads (app data only)
2017-07-16T15-00-03: app_stoc = server to client bytes delta excluding overheads (app data only)
2017-07-16T15-00-03: loss = number of packets lost. Can indicate lags.  Some node on the network is dropping packets or taking to long and we have to resend them.
2017-07-16T15-00-03: sent = number of packets sent. Spikes can indicate lag.
2017-07-16T15-00-03: ping = how long it takes for a packet to get back and forth. Spikes can indicate lag.
2017-07-16T15-00-03: variance = how much the ping is changing from avg ping. Spikes can indicate lag.
2017-07-16T15-00-03: reliable delayed = This occurs when we drop reliable packets from sending this frame because we are sending to much data. Unreliable are more likely to be dropped than reliable.
2017-07-16T15-00-03: unreliable delayed = This occurs when we drop unreliable packets from sending this frame because we are sending to much data.
2017-07-16T15-00-03: app update delayed = This occurs when the app is taking to long to run code caused by network packets (ie CPU) and packets are delayed until the next frame
2017-07-16T15-00-03: Time spent in critical section (frame) = This is the time the network thread is blocking the main thread from doing anything.
2017-07-16T15-00-03: Latency in Window = The average Latency in ms. of Reliable packets during this time slice
2017-07-16T15-00-03: Packet Loss % in Window = The packet loss % of Reliable packets during this time slice
2017-07-16T15-00-03: Jitter in Window = The average Jitter in ms. of Reliable packets during this time slice
2017-07-16T15-00-03: Overall Latency Min = The lowest Latency seen in ms. of Reliable packets up to this point in time
2017-07-16T15-00-03: Overall Latency Max = The largest Latency seen in ms. of Reliable packets up to this point in time
2017-07-16T15-00-03: Latency Min in Window = The lowest Latency seen in ms. of Reliable packets during this time slice
2017-07-16T15-00-03: Latency Max in Window = The largest Latency seen in ms. of Reliable packets during this time slice
2017-07-16T15-00-03: Latency packet samples = number of packets used in determining average latency from start of game
2017-07-16T15-00-03: Jitter packet samples = number of packets used in determining average jitter from start of game
2017-07-16T15-00-03: reconnect = flag to indicate one or more reconnects occurred
2017-07-16T15-00-03: [time], [address], [incoming], [outgoing], [app_ctos], [app_stoc], [loss], [sent], [ping], [variance], [reliable delayed], [unreliable delayed], [app update delayed], [Time spent in critical section (frame)], [Latency in Window], [Packet Loss % in Window], [Jitter in Window], [Overall Latency Min], [Overall Latency Max], [Latency Min in Window], [Latency Maxin Window], [Latency packet Samples], [Jitter Packet Samples],[reconnect]
1904,X.X.X.X,150,122,0,0,0,4,344,207,0,0,0,0,23,0.000000,0,23,24,23,24,3,2,1
14800,X.X.X.X,10085,2078,0,0,0,37,30,9,0,0,0,0,23,0.000000,0,23,24,23,24,36,31,0
24948,X.X.X.X,12259,2688,0,0,0,57,30,7,0,0,1,0,23,0.000000,0,23,24,23,24,55,50,0
34949,X.X.X.X,12923,3345,0,0,0,76,29,7,0,0,1,0,23,0.000000,0,22,24,22,24,75,68,0
44950,X.X.X.X,13569,4247,0,0,0,95,29,7,0,0,1,0,23,0.000000,0,22,24,22,24,94,87,0
54951,X.X.X.X,14215,5149,0,0,0,114,29,7,0,0,1,0,23,0.000000,0,22,24,23,23,113,106,0
64952,X.X.X.X,14861,6028,0,0,0,133,29,7,0,0,1,0,23,0.000000,0,22,24,23,24,132,125,0
74953,X.X.X.X,15507,6930,0,0,0,152,29,7,0,0,1,0,23,0.000000,0,22,24,23,24,151,144,0
84954,X.X.X.X,16153,7832,0,0,0,171,29,7,0,0